NTHU/NTU Light-field Camera (DragonFly) Dataset: Flower


Filelist:
  Sensor Image/P1010574.jpg - The captured image on the sensor

  5x5/xx_yy.png - The rectified 5x5 sparse light-field images (cropped and rectified from RAW image)

                  Naming rule: 
                      xx_06.png ~ xx_10.png (views from left to right)
                      06_yy.png ~ 10_yy.png (views from top to bottom)
      
                      For example, 08_08.png is the central view, and 06_10.png is the top-right view.


Note: Because the supporting ring is put deeply inside the camera, the surrounding views suffer occlusion from the flange.
      Our central-view-based algorihtms can handle this effect without modification.